# Facades after x years

|  |  |
| --- | --- |
| **Categories** |  |

**2004 and 2011 painted with** [**ThermoProtect**](https://www.climatecoating.com/en/products/thermoprotect/)**. No more mold.** The facade was last painted with [ClimateCoating® ThermoProtect](https://www.climatecoating.com/en/products/thermoprotect/) in 2011. Previously required to be repainted annually. Among other things, because of moisture problems and cracks due to traffic. In addition, the façade was equipped with the Schrijver system (ventilation slots).

### Metadata

|  |  |
| --- | --- |
| **qode\_animate-page-title** | no |
| **qode\_choose-number-of-portfolio-columns** | 3 |
| **qode\_content\_top\_padding** | 54 |
| **qode\_page\_subtitle** | Check out our work |
| **qode\_portfolio\_date** | June 02, 2014 |
| **qode\_portfolio\_type\_masonry\_style** | default |
| **qode\_show-page-title-image** | no |
| **qode\_show-page-title-text** | no |
| **qode\_choose-portfolio-image-size** | full |
| **qode\_portfolio-external-link-target** | \_self |
| **qode\_portfolio-image-gallery** | 22163,22165,22167,22169,22171 |
| **qode\_portfolio\_masonry\_parallax** | no |
| **qode\_portfolio\_show\_sidebar** | default |
| **vc\_teaser** | Array |
| **qode\_choose-portfolio-list-page** | 21923 |