# Up to 91.4% sunlight reflection! Cooler roofs thanks to ThermoActive roof coating

|  |  |
| --- | --- |
| **Categories** |  |

### Metadata

|  |  |
| --- | --- |
| **cmplz\_hide\_cookiebanner** |  |
| **qode\_slide-background-type** | image |
| **qode\_slide-bottom-right-alignment** | no |
| **qode\_slide-button-target** | \_self |
| **qode\_slide-button-target2** | \_self |
| **qode\_slide-content-alignment** | center |
| **qode\_slide-content-animation** | all\_at\_once |
| **qode\_slide-content-bottom** | 10 |
| **qode\_slide-content-right** | 0 |
| **qode\_slide-content-width** | 50 |
| **qode\_slide-contnet-fading-out** | fading\_out\_on |
| **qode\_slide-graphic-alignment** | center |
| **qode\_slide-hide-shadow** | yes |
| **qode\_slide-hide-title** | yes |
| **qode\_slide-image** | https://www.climatecoating.com/wp-content/uploads/2021/04/ThermoActive\_Roof\_SK\_1920x500px.jpg |
| **qode\_slide-separate-text-graphic** | no |
| **qode\_slide-subtitle** | Up to 91.4% sunlight reflection!<br>Cooler roofs thanks to ThermoActive roof coating |
| **qode\_slide-subtitle-font-family** | -1 |
| **qode\_slide-subtitle-font-size** | 36 |
| **qode\_slide-subtitle-line-height** | 38 |
| **qode\_slide-text-font-family** | -1 |
| **qode\_slide-thumbnail-animation** | flip |
| **qode\_slide-title-font-family** | -1 |
| **qode\_slide-vertical-alignment** | yes |